RustDesk server

Change ports of RustDesk server

The default ports are:

HBBR: 21117(TCP), 21119(TCP)

HBBS: (21114) API, 21115(TCP), 21116(UDP/TCP), 21118(TCP)

Thereby RustDesk requires more than one port and a specific port gets specified via -p, RustDesk takes the ports around this port:

Example:

HBBR: 55002, 55004

HBBS: (54999) API, 55000, 55001, 55003

Change ports with in system service:

ExecStart=/opt/rustdesk/hbbr -p55002

ExecStart=/opt/rustdesk/hbbs -p55001